Specimen data for CAM For this you require an Internet connection.

Specimen data for CAM for download.
| Wertheim.zip Description for the creation of a front plate using sample data with data creation in the graphic layers and direct export using the layer tool (simple data creation).
| Seitenregister.zip Description for the creation of a front plate with data creation in the milling layer, using sample data.
| Fräsarbeit_2D.zip Description of a 2D milling task with data creation in the milling layer, using sample data.
| Schild+RAHMEN.zip Description for the creation of a label with graphics and cutout with data creation in the milling layer, using sample data.
| BeschriftFette.zip Description for the creation of a circular inscription for component marking with data creation in the milling layer, using sample data.
| ErhabeneSchrift.zip Description for the creation of embossed lettering, using sample data.
| Engadin.zip Work specification and sample data label with recessed lettering (complex 2D milling processing at various depths, countersunk outline lettering using 2 tools, supporting lands and cutting out in layers) created using eSIGN2D. Nov. 2008
| Anfahrbewegung.zip Work specification and sample data, 3D approach movement (cutout milling paths with 3D approach movements and in layers) created using eSIGN2D(v3). Jan. 2009
| Maddy_50x67.9mm Description for the milling of a relief from photo, using sample data. Milling data output using eSIGN2D.
| Kurzanleitung.pdf Instructions Milling/Engraving Program eSIGN2D Instructions for data creation using eSIGN2D in German in pdf format for Adobe Acrobat.
Older work specifications using sample for eSIGN2D: Schild_040714.zip Description 'Input simple label' in Winword format using sample data (153kB) Required program configuration: HCAM / eSIGN2D Frontplatte_040714.zip Description 'Input small front plate' in Winword format with example (117kB) Required program configuration: HCAM / eSIGN2D Bahnsort.zip Description 'Sorting of the milling/engraving sequence' in Winword format with example (231kB) Required program configuration: HCAM / eSIGN2D Rundstempel_040714.zip Description 'Cutout circular stamp using BAZ engraved on cylinder' in Winword format with example (678kB) Required program configuration: HCAM / eSIGN3Di / eSIGN Art.
You require an internet connection! To load the data click-on the data using the right Mouse key <R> on the description (e.g. Wertheim.zip) and select Save under. After this the display File download. Here select Save and the target directory on your harddisk.