Sample data for Relief For this you require an Internet connection.

Sample data relief to download. All parts have been designed and calculated using ReliefVTR.
Aschenbecher.HRP (1.) Aschenbecher.JPG (2.) Aschenbecher.zip (3.) | Blume_HuM.HRP (1.) Blume_HuM.JPG (2.) Blume_HuM.zip (3.) | Eichel.HRP (1.) Eichel.JPG (2.) Eichel.zip (3.)
Fasnacht.HRP (1.) Fasnacht.JPG (2.) Fasnacht.zip (3.) | Fisch.HRP (1.) Fisch.JPG (2.) Fisch.zip (3.) | Glueck.HRP (1.) Glueck.JPG (2.) -
Sohle0.HRP (1.) Sohle0.JPG (2.) Sohle0.zip (3.) | Sohle3.HRP (1.) Sohle3.JPG (2.) Sohle3.zip (3.) | Sohle11.HRP (1.) Sohle11.JPG (2.) Sohle11.zip (3.)
Pocahontas.HRP (1.) Pocahontas.JPG (2.) Pocahontas.zip (3.) | Taube.HRP (1.) Taube.JPG (2.) - |
You require an Internet connection! To load the data click-on the description below the respective image (e.g. Ashtray.HRP). If an Internet connection exists, the display File download appears. Here, select Save and the target directory on your harddisk.
1 | Relief data in HRP format. The data can be loaded in the Relief program using Relief file . Relief open. Relief data are saved in the original dimensions an d in the highest quality (Recommended data format).
2 | Image data in JPG format. The data can be loaded in the Relief program using Relief file . Relief import . Photo. Image data receive no exact depth information. The Z resolution is limited to 256 levels.
3 | Shape data in STL format. The data can be loaded in the Relief program using Relief file . Relief import . STL. STL, due to the amount of data, is not very suitable for detailed Relief data. With coarser resolution a bevelling is quickly recognisable. Therefore, due to the quantity of data, usually in limited quality. Please unpack the files using WinZip.