Relief generation using CorelDRAW. To download the sample data you require an Internet connection.

Contents: Relief generation using CorelDRAW. Penthouse. Frame. 3D Corel. Graphic Corel. Experience. Sample data for Relief for download.

Relief generation using CorelDRAW. Using CorelDRAW you can generate graphics (photos) using grey shades. For this contours are provided (filled) using grey shades and grey progressions and integrated in images. The graphic created is exported in an image file using CorelDRAW, imported in the Relief program as photo and further processed into milling data for your machine. For the input in CorelDRAW knowledge of the operation of CorelDraw is presumed. The examples contain data for download. You require an Internet connection for the file download! To load the data click-on Sample data... if an Internet connection exists the indication file download appears. Here select Save and the target directory on your harddisk. Below are some examples with description of the procedure. Penthouse. 3D graphic from contours and lines.
| Create 2Dgraphic.
| In CorelDRAW, using the aid Filling provide contours with colour progressions. Save the finished graphic in an image file (BMP, JPG). Resolution e.g. 300dpi. Probe data in RelPenthouse.zip (Penthouse.cdr, Penthouse.jpg).
| Import graphic into Relief program using Relief File . Relief Import . Photo. As required the image can be smoothed using Relief Edit . filter (approximate). Using Relief Edit . mirror+rotate the relief can be brought into the required position (embossed, incised, shape etc.).
| Calculate milling paths using Relief AutoCorr and save in the format of the machine using PLayer Export.
Frame. 3D graphic from contours and lines.
| Create 2D graphic.
| In CorelDRAW, using the aid Filling provide contours with colour progressions. Save the finished graphic in an image file (BMP, JPG). Resolution e.g. 300dpi. Probe data in RelFrame.zip (Frame.cdr, Frame.jpg).
| Import graphic into Relief program using Relief File . Relief Import . Photo. As required the image can be smoothed using Relief Edit . filter (approximate). Using Relief Edit . mirror+rotate the relief can be brought into the required position (embossed, incised, shape etc.).
| Calculate milling paths using Relief AutoCorr and save in the format of the machine using PLayer Export.
3DCorel. 3D graphic contours and lines.
| In CorelDRAW, using the aid Filling provide contours with colour progressions. Save the finished graphic in an image file (BMP, JPG). Resolution e.g. 300dpi. Sample data in Rel3DCorel.zip (3DCorel.cdr, 3DCorel.jpg).
| Import graphic into Relief program using Relief File . Relief Import . Photo. As required the image can be smoothed using Relief Edit . filter (approximate). Using Relief Edit . mirror+rotate the relief can be brought into the required position (embossed, incised, shape etc.).
| Calculate milling paths using Relief AutoCorr and save in the format of the machine using PLayer Export.
Gra phic Corel. 3D graphic from contours, lines and integrated photo.
| Provide image (e.g. scan-in).
| Create supplementary 2D graphic. In CorelDRAW, using the aid Filling provide contours with colour progressions. Save the finished graphic in an image file (BMP, JPG). Resolution e.g. 300dpi. Sample data in RelGraphicCorel.zip (GraphicCorel.cdr, GraphicCorel.jpg).
| Import graphic into Relief program using Relief Datei . Relief Import . Photo. As required the image can be smoothed using Relief Edit . filter (approximate). Using Relief Edit . mirror+rotate the relief can be brought into the required position (embossed, incised, shape etc.).
| Calculate milling paths using Relief AutoCorr and save in the format of the machine using PLayer Export.
Experience. Lettering from contours at various levels and in 3D.
| Create 2D graphic.
| In CorelDRAW, using the aid Filling provide contours with colour progressions. Save the finished graphic in an image file (BMP, JPG). Resolution e.g. 300dpi. Sample data in RelExperience.zip (Experience.cdr, Experience.jpg).
| Import graphic into Relief program using Relief File . Relief Import . Photo. As required the image can be smoothed using Relief Edit . filter (approximate). Using Relief Edit . mirror+rotate the relief can be brought into the required position (embossed, incised, shape etc.).
| Calculate milling paths using Relief AutoCorr and save in the format of the machine using PLayer Export.

Sample data for Relief for download. All files are saved in jpg format as grey shade image. The images can, for example, be supplemented in CorelDRAW, imported into the Relief program as grey shade images and from which 3D milling paths are calculated. For download click-on the name under the graphic.
Ashtray | Bear | Cover | Knob
DotCircle | DotCircleBorderInv | Dot CircleBorder | Label0
Label 1 | Label2 | Label3 | WaveWasher
Ellipse | P retzel | Heart | Heart2
Star | Glasses | Gr eeting | Wedding
Flower | Card 1 | Card2 | Dove
Mark0 | Mark6 | Mark8 | MarkF0
MarkF10 | Pattern1 | Pattern2 | Frame1
Frame 2 | Frame art | Football | Gymnast
AJS | Altenst1 | Altenst2 | Bach
Bahrain | GerEagle1 | GerEagle 2 | Dragon
Acorn | AcornGriffon | Erfurt | Fish
Griffon | Guaranteed | Crown | Landau
Stone man | Unicorn | Escutcheon | Adornment
Angel | Block | Candle1 | Candle2
Candle 3 | Candle4 |  |